There are three parts need to do when going to use mBot’s Bluetooth with mBlock: 1. Upgrade firmware for mBot with USB cable; 2. Remove the USB cable and connect with Bluetooth; 3.Program for mBot wirelessly. Please view the video in this link for detailed steps: <https://www.youtube.com/watch?v=FxAsufUNcII>

**Note:** The steps in video take **Windows** PC as example, if you have a **Mac** PC, need note some differences while upgrading firmware and connecting the Bluetooth.

Before you upgrade firmware, need install a driver for Mac, here is the link to download the driver: <http://blog.sengotta.net/wp-content/uploads/2015/11/CH34x_Install.zip>

When choose Serial port under Connect->Serial Port, please choose the port similar to **/dev/tty.wchusbserial1410**.

As for connecting the Bluetooth, please refer to FAQ ‘**How to connect the bluetooth of my makeblock to Mac ?**’